**EL PRIMERO A386 REVIVAL**

**Iconic trio**

**Zenith sets the crowning touch to the festivities honouring its legendary 1969 El Primero high-frequency chronograph with a solid gold "revival" trilogy. The 38 mm case of this watchmaking icon, which is celebrating half a century of avant-garde and precision, appears clothed in this precious metal. To mark this anniversary, the three unisex models in white, rose or yellow gold are issued in 50-piece limited editions with a 50-year guarantee.**

El Primero has been writing the epic Zenith saga since 1969. For this golden jubilee, the world's most accurate automatic chronograph arrays its original attributes in the radiant glow of white, pink or yellow gold. Its revolutionary mechanics capable of tenth-of-a-second measurement, together with its three emblematic counters, have made it a legend. A cadence of 36,000 vibrations per hour; an integrated column-wheel construction; a ballbearing-mounted central rotor; and over 50 hours of power reserve (a real feat for such a high frequency) have been the signature features of El Primero creations for half a century. As a fitting tribute, Zenith presents three 50-piece re-editions of the original model, complete with a 50-year guarantee ensuring the bright future and heirloom stature of this anniversary series.

**Living legend**

Apart from its precious metal, this anniversary edition faithfully reproduces the initial characteristics of the 1969 El Primero: a 38 mm diameter case, a domed crystal, three-coloured counters, a tachymeter scale, as well as the shape of the hands and hour-markers. The mushroom-type pushers and lugs are also identical to the original, thanks to the "reverse engineering" process adopted. In designing this vintage series, each component of an original El Primero chronograph was digitised so as to ensure accurate reproduction of its properties. The only exceptions are the initially closed caseback that now fully reveals the movement, as well as the updated logo adorning the crown. Meanwhile, this model’s ‘engine’ is the current version of the El Primero automatic calibre powering the hours, minutes, small seconds, chronograph, tachymeter and date functions, with the latter appearing between 4 and 5 o’clock on the white lacquered dial. Nods to the past continue with a brown or black leather strap depending on the model – pictured here in rubber-lined alligator leather – fitted with a buckle made of the same gold as the case, as well as with the composition of the case. The latter contains a bright red travel pouch, like the one from 1969, as well as a microfibre cloth adorned on one side with an El Primero chronograph movement plan and on the other with a picture of the original user manual.

**ZENITH: the future of Swiss watchmaking**

Since 1865, Zenith has been guided by authenticity, daring and passion in pushing the boundaries of excellence, precision and innovation. Soon after its founding in le Locle by visionary watchmaker Georges Favre-Jacot, Zenith gained recognition for the precision of its chronometers, which it has won 2,333 chronometry prizes in just over a century and a half of existence: an absolute record. Famed for its legendary 1969 El Primero calibre enabling short-time measurement accurate to the nearest 1/10th of a second, Zenith has since developed over 600 movement variations. Today, Zenith offers new and fascinating vistas, including 1/100th of a second timing with the Defy El Primero 21. Energised by newly reinforced ties with a proud tradition of dynamic, avant-garde thinking, Zenith is writing its future… and the future of Swiss watchmaking.

**PRESS ROOM**

For additional pictures please access the below link

[**http://pressroom.zenith-watches.com/login/?redirect\_to=%2F&reauth=1**](http://pressroom.zenith-watches.com/login/?redirect_to=%2F&reauth=1)

**EL PRIMERO A386 REVIVAL**

TECHNICAL DETAILS

Reference: 65.A386.400.69.C815

**KEY POINTS**

Revival of the first ever El Primero Model from 1969

Original revival of the case with 38 mm diameter

Automatic El Primero column-wheel chronograph

White gold version: Limited Edition of 50 units

50 Years of Warranty

**MOVEMENT**

El Primero 400, Automatic

Calibre: 13 ¼ ``` (Diameter: 30 mm)

Movement thickness: 6.6.mm

Components: 278

Jewels: 31

Frequency: 36,000 VpH (5 Hz)

Power-reserve: min. 50 hours

Finishes: Oscillating weight with “Côtes de Genève”. motif

**FUNCTIONS**

Hours and minutes in the centre

Small seconds at 9 o'clock

Chronograph:

- Central chronograph hand

- 12-hour counter at 6 o'clock

- 30-minute counter at 3 o'clock

Tachymetric scale

Date indication at 4:30

**CASE, DIAL & HANDS**

Diameter: 38 mm

Diameter opening: 33.05 mm

Thickness: 12.60 mm

Crystal: Domed sapphire crystal with anti-reflective treatment on both sides

Case-back: Transparent sapphire crystal

Material: White gold

Water-resistance: 10 ATM

Dial: White-lacquered dial with three different-coloured counters

Hour-markers: Rhodium-plated, faceted and coated with Super-LumiNova SLN C3

Hands: Rhodium-plated, faceted and coated with Super-LumiNova SLN C3

**STRAP & BUCKLE**

Black alligator leather strap with protective rubber lining

White gold pin buckle

**EL PRIMERO A386 REVIVAL**

TECHNICAL DETAILS

Reference: 18.A386.400/69.C807

**KEY POINTS**

Revival of the first ever El Primero Model from 1969

Original revival of the case with 38 mm diameter

Automatic El Primero column-wheel chronograph

Rose gold version: Limited Edition of 50 units

50 Years of Warranty

**MOVEMENT**

El Primero 400, Automatic

Calibre: 13 ¼ ``` (Diameter: 30 mm)

Movement thickness: 6.6.mm

Components: 278

Jewels: 31

Frequency: 36,000 VpH (5 Hz)

Power-reserve: min. 50 hours

Finishes: Oscillating weight with “Côtes de Genève”. motif

**FUNCTIONS**

Hours and minutes in the centre

Small seconds at 9 o'clock

Chronograph:

- Central chronograph hand

- 12-hour counter at 6 o'clock

- 30-minute counter at 3 o'clock

Tachymetric scale

Date indication at 4:30

**CASE, DIAL & HANDS**

Diameter: 38 mm

Diameter opening: 33.05 mm

Thickness: 12.60 mm

Crystal: Box sapphire crystal with anti-reflective treatment on both sides

Case-back: Transparent sapphire crystal

Material: Rose gold

Water-resistance: 10 ATM

Dial: White-lacquered dial with three different-coloured counters

Hour-markers: Gold-plated, faceted and coated with Super-LumiNova SLN C3

Hands: Gold-plated, faceted and coated with Super-LumiNova SLN C3

**STRAP & BUCKLE**

Brown alligator leather strap with protective rubber lining

Rose gold pin buckle

**EL PRIMERO A386 REVIVAL**

TECHNICAL DETAILS

Reference: 30.A386.400/69.C807

**KEY POINTS**

Revival of the first ever El Primero Model from 1969

Original revival of the case with 38 mm diameter

Automatic El Primero column-wheel chronograph

Yellow gold version: Limited Edition of 50 units

50 Years of Warranty

**MOVEMENT**

El Primero 400, Automatic

Calibre: 13 ¼ ``` (Diameter: 30 mm)

Movement thickness: 6.6.mm

Components: 278

Jewels: 31

Frequency: 36,000 VpH (5 Hz)

Power-reserve: min. 50 hours

Finishes: Oscillating weight with “Côtes de Genève”. motif

**FUNCTIONS**

Hours and minutes in the centre

Small seconds at 9 o'clock

Chronograph:

- Central chronograph hand

- 12-hour counter at 6 o'clock

- 30-minute counter at 3 o'clock

Tachymetric scale

Date indication at 4:30

**CASE, DIAL & HANDS**

Diameter: 38 mm

Diameter opening: 33.05 mm

Thickness: 12.60 mm

Crystal: Box sapphire crystal with anti-reflective treatment on both sides

Case-back: Transparent sapphire crystal

Material: Yellow gold

Water-resistance: 10 ATM

Dial: White-lacquered dial with three different-coloured counters

Hour-markers: Gold-plated, faceted and coated with Super-LumiNova SLN C3

Hands: Gold-plated, faceted and coated with Super-LumiNova SLN C3

**STRAP & BUCKLE**

Brown alligator leather strap with protective rubber lining

Yellow gold pin buckle